# EEA marine assessment grid, Jan. 2017

This metadata refers to the EEA marine assessment grid, to which all data and assessment results have been spatially mapped in order to ensure that data can be compared in a uniform way across the European regional seas.

The marine assessment grid is based on the EEA reference grid system. The EEA reference grid is based on ERTS89 Lambert Azimuthal Equal Area projection with parameters: latitude of origin 52° N, longitude of origin 10° E, false northing 3 210 000.0 m, false easting 4 321 000.0 m. All grid cells are named with a unique identifier containing information on grid cell size and the distance from origin in meters (easting and northing). An important attribute of the EEA reference grid system is that by using an equal area projection all grid cells are having the same area for the same grid size. 

In this marine assessment grid, two grid sizes are used:
* 100 x 100 km in offshore areas (> 20 km from the coastline)
* 20 x 20 km in coastal areas (<= 20 km from the coastline)
The grid sizes were choosen after an evaluation of data availability versus the need for sufficient detail in the resulting assessment. The resulting assessment grid is a combination of two grid sizes using the EEA reference grid system.

The overall area of interest used in the grid is based on the marine regions and subregions under the Marine Strategy Framework Directive (MSFD). Additionally, Norwegian (Barent Sea and Norwegian Sea) and Icelandic waters (’Iceland Sea’) have been added (see Surrounding seas of Europe). Note that, within the North East Atlantic region, only the subregions within EEZ boundaries (~200 nm) have been included.https://sdi.eea.europa.eu/geonetwork/srv/api/records/84d1f816-1913-45b1-94b7-a5721a18296c


[More information](https://sdi.eea.europa.eu/catalogue/srv/api/records/84d1f816-1913-45b1-94b7-a5721a18296c)
    