# Hillshade Europe DEM

This is a cropped DTM version (with Frame2c) for providing topographic backgrouds on EEA maps.
This is a hillshade of global digital elevation model (DEM) with a horizontal grid spacing of 30 arc seconds (approximately 1 kilometer).https://sdi.eea.europa.eu/geonetwork/srv/api/records/84036394-19fc-466f-bc4b-b0748d5d29f4


[More information](https://sdi.eea.europa.eu/catalogue/srv/api/records/84036394-19fc-466f-bc4b-b0748d5d29f4)
    